After V23 has a model with the switched shunts from the raw and Powerworld cases represented in MATPOWER as generators rather than as fixed impedance loads.

Also, there were a few buses in V22 with multiple generators at the same bus and the distribution of generation resulted in a few minimum limits being violated. This was corrected in V23.

Finally, several zero flow ties buses were reset to have non-zero but small flows.